

Mouse User's Manual


1994-2001 Copyright All Rights Reserved
FCC Statement on CLASS B

  Note: This equipment has been tested and found to comply with the limits  for
  a CLASS B digital device, pursuant to Part 15 of the FCC Rules. These  limits
  are designed to provide reasonable protection  against  harmful  interference
  when the equipment is operated in a residential installation. This  equipment
  generates, uses, and can radiate radio frequency energy and if not  installed
  and used  in  accordance  with  the  instruction  manual  may  cause  harmful
  interference  to radio  communications.  However, there is no guarantee  that
  interference   will  not  occur  in  a  particular   installation.   if  this
  equipment does cause interference to radio or television reception, which can
  be  determined   by  turning   the  equipment   off  and  on,  the  user   is
  encouraged to try to correct the interference by one or more of the following
  measures:

  * Reorient  or relocate  the  receiving  antenna.
  * Increase  the separation between the equipment and receiver.
  * Connect the equipment into an outlet on a circuit different from that to
    which the receiver is connected.
  * Consult the dealer or an experienced radio TV technician for help.


  This device complies with Part 15 of the FCC Rules. Operation is subject to
  the following two conditions:

  (1) this device may not cause harmful interference.

  (2) this device must accept any interference received, including
      interference that may cause undesired operation.


1. Hardware Installation
 1-1.Installing a Serial Mouse
     You must have a PC fitted with a serial port(COM1/COM2) in order to
     install the mouse. Plug your mouse into the serial port.

 1-2.Installing a Mouse with Mouse Port (PS/2) Connector
     If you have a mouse with a round mouse port connector, you must turn off
     the computer before connecting or disconnecting your mouse.

 1-3.Installing a Combo Mouse
     The Combo Mouse comes with a PS/2 (DIN 6) cable connector, together with
     a PS/2 -> Serial (COM 9) port adapter.
     Before plug your mouse into the computer, try to make sure what kind of
     mouse port you have. If you have a PS/2 port, plug in the original PS/2
     cable connector; if you have a Serial port, please connect the adapter
     first to the cable, then plug into the Serial port.
       1. Turn the computer off.
       2. Locate an available 6-pin round port on your computer.
       3. Insert the mouse connector into the round mouse port.
       4. Start your computer.

 1-4.Installing a USB Mouse
     When you use a mouse with USB connector , you don't have to shut off the 
     computer. Just plug the USB connector into the USB port

 

2. Mouse Driver Installation

  Mouse software supports Windows 95, Windows 98, Windows ME,
  Windows NT 4.0, Windows 2000 and Windows XP.
  
  Before installing any software under Windows NT 4.0, we
  strongly recommend you create an Emergency Repair Disk using
  the Repair Disk utility provided by the system (RDISK.EXE).
  
  Please note that USB mice are only supported under Windows 98, Windows ME,
 Windows 2000, and Windows XP. 
   
  Run Setup.exe to install the Mouse software.  
 

3. Uninstall Program
  
  Mouse Software can be removed from Windows by
  clicking the Add/Remove Programs icon in the Control Panel or clicking
  the "Uninstall" icon in the folder that setup.exe created in "Programs" 
  of "Start" button on Windows desktop.
  Select Mouse Software installed and click the "Remove" button.   
 
4. Switching Mouse Mode
 4-1.Switching Mouse Hareware Modes (Use mode switch)
     The Serial Mouse is capable of operating either as a Microsoft Serial
     Mouse or a Mouse Systems Mouse. At the base of the Mouse you will find a
     slide switch. The switch has two possible positions, 'MS' and 'PC' When
     the switch is set to the 'MS' position the Mouse will emulate a two-buttoned
     Microsoft Mouse while setting the switch to the 'PC' position will cause
     the Mouse to emulate a three-buttoned Mouse Systems Mouse.


 4-2.Switching Mouse Hardware Modes (None mode switch)
     As mentioned earlier, the serial mouse is capable of operating either as
     a Microsoft Serial Mouse or a Mouse Systems Mouse. Which of the two modes
     the mouse will operate in is determined on the power-on initialization.
     If any one of the three buttons is depressed during power-on initializa-
     tion, the mouse will emulate Mouse Systems Mouse. While none of the
     buttons is depressed during power-on initiation the mouse will emulate
     Microsoft Mouse.

 4-3.Microsoft Mode
     When the mouse is in Microsoft mode, only the left and right buttons are
     active, while the middle button is ignored. In this mode, your mouse will
     correctly emulate a Microsoft Serial Mouse.

 4-4.Mouse Systems Mode
     If you are a user of AUTOCAD or any other software which gives enhanced
     performance with a Mouse Systems Mouse you should choose this emulation.
     A Mouse Systems Mouse operates with all three buttons.

 Note: Because Windows 95 and Windows NT supports serial 'MS' mouse mode, you
       had better switch the mouse to 'MS' mode when first install the mouse
       driver in package. After completing the installation, you can switch
       to 'PC' mouse mode when restart the computer.


5. Trouble Shooting

Symptom 1 : No mouse movement.
Solution  : - Make sure the software that you are using supports a mouse.
            - Check that mouse is plugged into serial port at the back of
              computer.
            - Ensure that mouse driver is installed into system.

Symptom 2 : The cursor on the screen remains at one spot or moves erratically.
Solution  : Check the mouse cable for any breaks or sharp twists. Examine the
            cable closely where it connects to the mouse.

Symptom 3 : The cursor movement stops at a corner and no longer responds to
            the mouse movement.
Solution  : Run the mouse driver to check which mode the mouse is operating in.

Symptom 4 : Mouse movement does not produce corresponding cursor movement or
            there is a brief pause during movement.
Solution  : Clean the silicon rubber-coated ball and rollers.

Symptom 5 : After had selected mouse type for Windows 95 ,the mouse would be
            disable when you clicked "OK" .
Solution  : Using keyboard to close the current window and wait for Windows 95
            to give any instruction to restart your computer.
            After restart Windows 95 the mouse will work normally.

Symptom 6 : Displayed error number -115 on screen when install mouse driver
            software.
Solution  : The error usually occurs because a virus-checking program is being
            used on the System to prevent files from being renamed. Please
            shutdown any virus checking software running on the system and
            then run the setup again.

Symptom 7 : Detection Problems with PS/2 Pointing Devices
Solution  : If your mouse is connected to the mouse port and is not detected
            by the system, attempt the following step(s):

            1) Your mouse port might need to be enabled through the SETUP menu
               of your computer. Please check your computer documentation
               regarding the SETUP menu.

            2) If you have a mouse with both serial and mouse port adaptors,
               connect the mouse to the computer through the serial port.
               Reboot and check if the mouse is detected properly.

            3) If adaptor(s) were not included in your package, your mouse
               was designed to work on only one type of port (Serial OR PS/2).
               Refer to your package for the type of port your mouse supports.
  
            If the problem persists, please check for a possible computer
            BIOS ROM upgrade from your computer manufacturer.
  
            Some notebook systems, such as IBM Thinkpad, have both an external
            Mouse Port and an integrated Pointing Stick, which is connected to
            the Mouse Port. If your mouse is having difficulty running on the
            Mouse Port of this type of system, try using the serial port
            instead.

Symptom 8 : Conflicts with other Serial Devices
Solution  : Some softwares provided by other manufacturers with mouse
            functions, such as Logitech MouseWare, which may conflict with
            this mouse. Recommended strongly to remove the software installed
            previously before install this mouse software.

Symptom 9 : Problems Operating the Wheel
Solution  : If your mouse is equipped with a wheel and the wheel does not
            scroll, verify the following:

            1) Verify that the "Browser Mouse" or "Mouse Control Panel"
               application is installed properly. If you do not find the
               "Browser Mouse" or "Mouse Control Panel" icon in the system
               tray, you need to reinstall mouse software.

            2) Some other applications with mouse scrolling function may
               conflict with this mouse function. Remove these applications
               before install this mouse software.

