The following registry keys are an example of what would be required to have your device install 
without user interaction.
To obtain a more accurate set of registry settings first install your device then extract the registry
settings from your target using Embedded Visual C++ registry editor or similar. The settings that are relevant 
are in the HKEY_LOCAL_MACHINE\Drivers\USB section.

[HKEY_LOCAL_MACHINE\Drivers\USB\FTDI_DEVICE_6001]
"Prefix"="COM"
"Dll"="ftdi_ser.dll"
"ConfigData"=hex:\
      01,00,3f,3f,10,27,88,13,c4,09,e2,04,71,02,38,41,9c,80,4e,c0,34,00,1a,00,0d,\
      00,06,40,03,80,00,00,d0,80
"InitialIndex"=dword:00000000
"DeviceArrayIndex"=dword:00000000
"LatencyTimer"=dword:00000010

[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\1027_24577\Default\Default\FTDI_DEVICE]
"DLL"="ftdi_ser.dll"