Features 
Integrated 10/100/1000 transceiver 
Auto-Negotiation with Next Page capability 
Supports PCI rev.2.3, 32-bit, 33/66MHz 
Supports pair swap/polarity/skew correction 
Crossover Detection & Auto-Correction 
Wake-on-LAN and remote wake-up support 
Microsoft? NDIS5 Checksum Offload (IP, TCP, UDP) and largesend offload support 
Supports Full Duplex flow control (IEEE 802.3x) 
Fully compliant with IEEE 802.3, IEEE 802.3u, IEEE 802.3ab 
Supports IEEE 802.1P Layer 2 Priority Encoding 
Supports IEEE 802.1Q VLAN tagging 
Serial EEPROM 
3.3/1.8/1.5V signaling, 5V PCI I/O tolerant 
0.15¦Ìm CMOS process 
Transmit/Receive FIFO (8K/64K) support 
Supports power down/link down power saving 
Supports PCI Message Signaled Interrupt (MSI) 
128-pin QFP package for RTL8169SC and 128-pin LQFP package for RTL8169SCL 
 
